# SLOG_PROF_AddExtraIntvlInfo

Add one display description of an interval to the reserved space of the SLOG Display Profile table.

## Synopsis

    int SLOG_PROF_AddExtraIntvlInfo(       SLOG_STREAM      *slog,
                                     const SLOG_intvltype_t  intvltype,
                                     const SLOG_bebit_t      bebit_0,
                                     const SLOG_bebit_t      bebit_1,
                                     const char *            classtype,
                                     const char *            label,
                                     const char *            color )

## Modified Input Variables

slog - pointer to the SLOG_STREAM where SLOG Display Profile Table is located.

## Unmodified Input Variables

intvltype - index to the interval type.

bebit_0 - the 1st bebit.

bebit_1 - the 2nd bebit.

classtype - character string for the classtype of the interval

label - character string for the label of the interval

color - character string for the color of the interval

## Modified Output Variables

returned value - integer return status.

## Usage Notes on this subroutine

all the input characters strings, classtype, label and color are allowed to contain alphanumeric, underscore, blank and tab characters. But tab characters, if exist, in the string are all converted to blanks for ease of management.

Notes on the Addition of Extra Interval Description. This note is to clarify the usage of SLOG_PROF_XXX() routines especially while the user wants to add extra interval description to the logfile when the process of addition of interval records to the logfile has been started, for instance if one needs to add user marker interval records.

Also, the term interval descriptor refers to an entry in the Display Profile, so is the term interval information, abbrev. as _IntvlInfo_. These 3 terms are used interchangably.

Under normal circumstances, the Display Profile table is created by first opening the section of the logfile for storing the table using SLOG_PROF_Open(). Then add the interval description using SLOG_PROF_AddIntvlInfo() and close the table section by SLOG_PROF_Close().

In the case that the logfile involves interval records whose interval type are NOT known until the process of inserting of the interval records to the logfile has been started, one should open the SLOG_PROF_Open(). Then add the known record definitions using SLOG_PROF_AddIntvlInfo(). However, one should NOT call SLOG_PROF_Close() to close the table section. Instead, SLOG_PROF_SetExtraNumOfIntvlInfos() should be called to set the extra number of interval description entries needed( the number can be greater than what one actually needs ). Then when user encounters a new interval record type, SLOG_PROF_AddExtraIntvlInfo() can then be called to add the new interval record type to the Display Profile table. This mechanism is very similar to that of Record Definition Table. Except for Record Definition Table, the above procedure has to be done before adding the interval record to the logfile using SLOG_Irec_ToOutputStream() which does NOT allow interval record of with unknown interval type to the Record Definition table. For Display Profile, the same procedure is implmented to simplify the interface for user to store interval description information to the logfile, the interval description information is NOT important till logfile needs to be displayed graphically.

## Include file needed

slog_profile.h

## Notes on SLOG return status code

There are 5 allowed SLOG returned status codes. They include SLOG_SUCCESS, SLOG_FAIL and SLOG_EOF. Their actual values are defined in slog.h

SLOG_SUCCESS is returned when no error is encountered.

SLOG_FAIL is returned when error is encounted.

SLOG_EOF is returned when End of file is encounted.

There are also SLOG_TRUE and SLOG_FALSE which are sued as boolean values, in particular they are used in boolean functions which are usually named as IsXXXXX(), AreXXXXX() and HasXXXXX().

Location:../src/slog_profile.c